#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\RAM_Function\RAMFunction.uvproj
    Project File Date:  07/26/2012

    Output:
    Build target 'Target 1'
    creating preprocessor file for RAMFunctionMain.c...
    compiling RAMFunctionMain.c...
    creating preprocessor file for Config.c...
    compiling Config.c...
    creating preprocessor file for RAMFunction.c...
    compiling RAMFunction.c...
    creating preprocessor file for LCD.c...
    compiling LCD.c...
    creating preprocessor file for LCD_b.c...
    compiling LCD_b.c...
    assembling Startup.s...
    linking...
    Program Size: Code=3544 RO-data=240 RW-data=1544 ZI-data=8292
    FromELF: creating hex file...
    ".\obj\RAMFunction.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\RAM_Function\\obj\\RAMFunction.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\RAM_Function\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.