Static Call Graph - [D:\МиландрНН\=EVAL KITS=\Eval Kit 1986ВЕ9X\CD_info\Отладочная плата 1986ВЕ91Т (94Т)\Модуль Ethernet\Проекты\ICMP_Parallel_5600VG1U\TestParallel5600VG1U.axf]

# Static Call Graph for image D:\МиландрНН\=EVAL KITS=\Eval Kit 1986ВЕ9X\CD_info\Отладочная плата 1986ВЕ91Т (94Т)\Модуль Ethernet\Проекты\ICMP_Parallel_5600VG1U\TestParallel5600VG1U.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 894]: Last Updated: Thu Apr 24 12:26:42 2014

### Maximum Stack Usage = 72 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ Answear_ARP ⇒ Write_Tx_Descriptor

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- AACI_IRQHandler ⇒ AACI_IRQHandler

  ### Function Pointers

  - AACI_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - BusFault_Handler from startup.o(.text) referenced from startup.o(RESET)
  - CAN_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - CHLCD_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - CLCD_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - DebugMon_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ENET_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - FLEXRAY_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - HardFault_Handler from startup.o(.text) referenced from startup.o(RESET)
  - I2C_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - LIN_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - MCIA_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - MCIB_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - MemManage_Handler from startup.o(.text) referenced from startup.o(RESET)
  - NMI_Handler from startup.o(.text) referenced from startup.o(RESET)
  - PendSV_Handler from startup.o(.text) referenced from startup.o(RESET)
  - RTC_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - Reset_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SPI_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - SVC_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SysTick_Handler from startup.o(.text) referenced from startup.o(RESET)
  - TIM0_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - TIM2_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - UART0_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - UART1_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - UART2_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - UART3_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - USBDC_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - USBHC_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - UsageFault_Handler from startup.o(.text) referenced from startup.o(RESET)
  - WDT_IRQHandler from startup.o(.text) referenced from startup.o(RESET)
  - __main from __main.o(!!!main) referenced from startup.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 90 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __decompress1 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> _fp_init
  [Called By]
  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_li ⇒ __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ Answear_ARP ⇒ Write_Tx_Descriptor
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  EthCfg (Thumb, 96 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  Write_Tx_Descriptor (Thumb, 84 bytes, Stack size 12 bytes, main.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Write_Tx_Descriptor
  [Called By]
  - >> Answear_ARP
  - >> Answear_ICMP

  Read_Tx_Descriptor (Thumb, 24 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> Answear_ARP
  - >> Answear_ICMP

  Ready_Rx_Descriptor (Thumb, 28 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  Read_Rx_Descriptor (Thumb, 24 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  Read_Packet_Length (Thumb, 12 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  Read_Packet_Start_Address (Thumb, 14 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  PortConfig (Thumb, 138 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  ClkCfg (Thumb, 36 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  CheckSum_ICMP (Thumb, 68 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CheckSum_ICMP
  [Called By]
  - >> main
  - >> Answear_ICMP

  CheckSum_IP (Thumb, 60 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CheckSum_IP
  [Called By]
  - >> main
  - >> Answear_ICMP

  Answear_ICMP (Thumb, 520 bytes, Stack size 20 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Answear_ICMP ⇒ Write_Tx_Descriptor
  [Calls]
  - >> CheckSum_IP
  - >> CheckSum_ICMP
  - >> Read_Tx_Descriptor
  - >> Write_Tx_Descriptor
  [Called By]
  - >> main

  Answear_ARP (Thumb, 474 bytes, Stack size 60 bytes, main.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = Answear_ARP ⇒ Write_Tx_Descriptor
  [Calls]
  - >> Read_Tx_Descriptor
  - >> Write_Tx_Descriptor
  [Called By]
  - >> main

  Read_Packet (Thumb, 92 bytes, Stack size 12 bytes, main.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Read_Packet
  [Called By]
  - >> main

  InitRxDescriptor (Thumb, 96 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  InitTxDescriptor (Thumb, 100 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  main (Thumb, 780 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = main ⇒ Answear_ARP ⇒ Write_Tx_Descriptor
  [Calls]
  - >> InitTxDescriptor
  - >> InitRxDescriptor
  - >> Read_Packet
  - >> Answear_ARP
  - >> Answear_ICMP
  - >> CheckSum_IP
  - >> CheckSum_ICMP
  - >> ClkCfg
  - >> PortConfig
  - >> Read_Packet_Start_Address
  - >> Read_Packet_Length
  - >> Read_Rx_Descriptor
  - >> Ready_Rx_Descriptor
  - >> EthCfg
  [Called By]
  - >> __rt_entry_main

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  AACI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> AACI_IRQHandler
  [Called By]
  - >> AACI_IRQHandler
  [Address Reference Count : 1]
  - startup.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  CHLCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  CLCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  FLEXRAY_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  I2C_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  LIN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  MCIA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  MCIB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  TIM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  USBDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  USBHC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __rt_fp_status_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_fp_status_addr_intlibspace.o(.text))
  [Called By]

  - >> _fp_init

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 8 bytes, indicate_semi.o(.text), UNUSED)

  _fp_init (Thumb, 14 bytes, Stack size 8 bytes, fpinit.o(x$fpl$fpinit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _fp_init
  [Calls]
  - >> __rt_fp_status_addr
  [Called By]
  - >> __rt_lib_init

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  ### Undefined Global Symbols