*** Creating Trace Output File 'Ethernet.tra' Ok.
### Preparing for ADS-LD.
### Creating ADS-LD Command Line
### List of Objects: adding '"main.o"'
### List of Objects: adding '".\startup_mps.o"'
### ADS-LD Command completed:
"main.o" ".\startup_mps.o" --device DLM --scatter "Ethernet.sct" 

--autoat --summary_stderr --info summarysizes --map --xref --callgraph --symbols 

--info sizes --info totals --info unused --info veneers 

 --list ".\Ethernet.map" -o "Ethernet.axf"### Preparing Environment (PrepEnvAds)
### ADS-LD Output File: 'Ethernet.axf'
### ADS-LD Command File: 'Ethernet.lnp'
### Checking for dirty Components...
### Creating CmdFile 'Ethernet.lnp', Handle=0x00000294
### Writing '.lnp' file
### ADS-LD Command file 'Ethernet.lnp' is ready.
### ADS-LD: About to start ADS-LD Thread.
### ADS-LD: executed with 0 errors
### Updating obj list
### LDADS_file() completed.
