#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\DAC_1\DACProject.uvproj
    Project File Date:  12/08/2011

    Output:
    Build target 'Target 1'
    assembling Startup.s...
    linking...
    .\obj\DACProject.axf: Warning: L6665W: Neither Lib$$Request$$armlib Lib$$Request$$cpplib defined, not searching ARM libraries.
    .\obj\DACProject.axf: Error: L6411E: No compatible library exists with a definition of startup symbol __main.
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=356 RO-data=208 RW-data=0 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    src\Config.c(2): error:  #5: cannot open source input file "EthFunc.c": No such file or directory
    compiling DACProjectMain.c...
    src\Config.c(2): error:  #5: cannot open source input file "EthFunc.c": No such file or directory
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    src\Config.c(44): warning:  #61-D: integer operation result is out of range
    src\Config.c(44): warning:  #68-D: integer conversion resulted in a change of sign
    linking...
    Program Size: Code=584 RO-data=208 RW-data=0 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 2 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    src\DACProjectMain.c(12): warning:  #223-D: function "NVIC_IRQEnable" declared implicitly
    linking...
    .\obj\DACProject.axf: Error: L6218E: Undefined symbol NVIC_IRQEnable (referred from dacprojectmain.o).
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=560 RO-data=208 RW-data=0 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1072 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1084 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1080 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1104 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1104 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1104 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1008 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1008 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1008 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=992 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=984 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=984 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=984 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=984 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=984 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=984 RO-data=224 RW-data=220 ZI-data=8292
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1088 RO-data=224 RW-data=220 ZI-data=8292
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    src\DACProjectMain.c(45): error:  #20: identifier "Sec" is undefined
    Target not created
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    _____^
    *** error 56: cant open file
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1072 RO-data=224 RW-data=216 ZI-data=8288
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\DAC_1\\obj\\DACProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\DAC_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    creating preprocessor file for DACProjectMain.c...
    compiling DACProjectMain.c...
    linking...
    Program Size: Code=1072 RO-data=224 RW-data=212 ZI-data=8292
    FromELF: creating hex file...
    ".\obj\DACProject.axf" - 0 Error(s), 0 Warning(s).