#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\Ethernet100BaseT_ICMP_Server.uvproj
    Project File Date:  12/01/2011

    Output:
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2246 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2246 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2246 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2246 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: Could not measure total IR len. TDO is constant high.
    **JLink Warning: CPU core not found.
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    **JLink Warning: Could not set S_RESET_ST
    **JLink Warning: CPU did not halt after reset.
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2254 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2254 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = ?, IRPrint = 0x..000000000000000000000000
    **JLink Warning: CPU core not found.
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #550-D: variable "tmp" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #550-D: variable "tmp" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2258 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(63): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2250 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(69): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2262 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(70): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2266 RO-data=218 RW-data=0 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(89): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2538 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(90): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2538 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2538 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(57): error:  #31: expression must have integral type
    src\Ethernet100BaseTMain.c(57): error:  #20: identifier "RXTX" is undefined
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    Target not created
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    _____^
    *** error 56: cant open file
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2550 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2558 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2558 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2558 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2550 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2550 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    linking...
    Program Size: Code=2562 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2562 RO-data=234 RW-data=12 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2610 RO-data=234 RW-data=16 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2570 RO-data=234 RW-data=16 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2582 RO-data=234 RW-data=16 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2610 RO-data=234 RW-data=16 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2646 RO-data=234 RW-data=16 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2670 RO-data=234 RW-data=20 ZI-data=8868
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2702 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(42): warning:  #61-D: integer operation result is out of range
    src\config.c(42): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(92): warning:  #177-D: variable "tmp" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2702 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2862 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2866 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2870 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2870 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2870 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2874 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: SYSRESETREQ has confused core. Trying to reconnect and use VECTRESET.
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    **JLink Warning: Could not set S_RESET_ST
    **JLink Warning: CPU did not halt after reset.
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(116): error:  #65: expected a ";"
    src\Ethernet100BaseTMain.c(127): warning:  #12-D: parsing restarts here after previous syntax error
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    Target not created
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2874 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2834 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 13 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2834 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 13 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2834 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 13 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2834 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 13 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2834 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 13 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2834 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 12 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2826 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 12 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(93): warning:  #550-D: variable "i" was set but never used
    assembling Startup.s...
    linking...
    Program Size: Code=2826 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 12 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(117): error:  #513: a value of type "unsigned char *" cannot be assigned to an entity of type "unsigned int *"
    assembling Startup.s...
    Target not created
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    _____^
    *** error 56: cant open file
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2894 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 12 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 12 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\config.c(77): warning:  #1-D: last line of file ends without a newline
    assembling Startup.s...
    linking...
    Program Size: Code=2866 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 11 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2866 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: SYSRESETREQ has confused core. Trying to reconnect and use VECTRESET.
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    ***JLink Error: Bad JTAG communication: Write to IR: Expected 0x1, got 0x0 (TAP Command : 10) @ Off 0x5.
    ***JLink Error: Target system has no power.
    **JLink Warning: CPU core not found.
    ***JLink Error: Can not read register 15 (R15) while CPU is running
    **JLink Warning: RESET (pin 15) high, but should be low. Please check target hardware.
    ***JLink Error: Wrong AHB ID (15:3). Expected 0x04770001 (Mask 0x0FFFFF0F), Found 0x00000000
    Could not read memory location 0x20100000 when trying to clear soft RAM BP
    ***JLink Error: Can not read register 20 (CFBP) while CPU is running
    Cannot setup Breakpoint at Address
    Full Chip Erase Failed!
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "i" was declared but never referenced
    src\Ethernet100BaseTMain.c(94): warning:  #177-D: variable "SMode" was declared but never referenced
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2770 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 14 Warning(s).
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "i" was declared but never referenced
    src\Ethernet100BaseTMain.c(94): warning:  #177-D: variable "SMode" was declared but never referenced
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2770 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 14 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2854 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=2954 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    assembling Startup.s...
    linking...
    Program Size: Code=3006 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 10 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "i" was declared but never referenced
    src\Ethernet100BaseTMain.c(94): warning:  #177-D: variable "SMode" was declared but never referenced
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2766 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 14 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "i" was declared but never referenced
    src\Ethernet100BaseTMain.c(94): warning:  #177-D: variable "SMode" was declared but never referenced
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2762 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 14 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling Ethernet100BaseTMain.c...
    src\EthFunc.c(164): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(181): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(183): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(139): warning:  #550-D: variable "space_start" was set but never used
    src\EthFunc.c(224): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(242): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(245): warning:  #767-D: conversion from pointer to smaller integer
    src\EthFunc.c(247): warning:  #767-D: conversion from pointer to smaller integer
    src\config.c(49): warning:  #61-D: integer operation result is out of range
    src\config.c(49): warning:  #68-D: integer conversion resulted in a change of sign
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "tmp" was declared but never referenced
    src\Ethernet100BaseTMain.c(93): warning:  #177-D: variable "i" was declared but never referenced
    src\Ethernet100BaseTMain.c(94): warning:  #177-D: variable "SMode" was declared but never referenced
    src\Ethernet100BaseTMain.c(95): warning:  #177-D: variable "Src" was declared but never referenced
    assembling Startup.s...
    linking...
    Program Size: Code=2774 RO-data=234 RW-data=24 ZI-data=8872
    FromELF: creating hex file...
    ".\obj\Ethernet100BaseT_ICMP_Server.axf" - 0 Error(s), 14 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\Ethernet_100BaseT_ICMP_Server\\obj\\Ethernet100BaseT_ICMP_Server.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\Ethernet_100BaseT_ICMP_Server\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.