#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\BatteryPowerProject.uvproj
    Project File Date:  10/10/2011

    Output:
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=496 RO-data=184 RW-data=8 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    src\BatteryPowerMain.c(3): error:  #18: expected a ")"
    src\BatteryPowerMain.c(3): error:  #70: incomplete type is not allowed
    src\BatteryPowerMain.c(3): error:  #70: incomplete type is not allowed
    src\BatteryPowerMain.c(3): error:  #65: expected a ";"
    src\BatteryPowerMain.c(13): warning:  #223-D: function "ClkConfig" declared implicitly
    src\BatteryPowerMain.c(15): warning:  #223-D: function "SysTickInit" declared implicitly
    src\BatteryPowerMain.c(24): error:  #28: expression must have a constant value
    src\BatteryPowerMain.c(29): error:  #28: expression must have a constant value
    src\BatteryPowerMain.c(38): error:  #159: declaration is incompatible with previous "ClkConfig" (declared at line 13)
    assembling Startup.s...
    Target not created
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    src\BatteryPowerMain.c(15): warning:  #223-D: function "SysTickInit" declared implicitly
    assembling Startup.s...
    linking...
    .\obj\BatteryPowerProject.axf: Error: L6218E: Undefined symbol SysTickInit (referred from batterypowermain.o).
    Target not created
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=628 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=660 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=660 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    linking...
    Program Size: Code=636 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=636 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=656 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=672 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=680 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=680 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=692 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=708 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=704 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=716 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=708 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=700 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=712 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.287V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=712 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=708 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=700 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=728 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=728 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=696 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=708 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=704 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=732 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=744 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=744 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=628 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=628 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=624 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=652 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=684 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.287V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=828 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=828 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=828 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=836 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=848 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=848 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=848 RO-data=208 RW-data=12 ZI-data=8292
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=880 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 0 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 0
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=832 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=832 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=820 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=816 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=704 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=720 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=828 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=812 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=848 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=848 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=860 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling BatteryPowerMain.c...
    assembling Startup.s...
    linking...
    Program Size: Code=860 RO-data=208 RW-data=16 ZI-data=8288
    ".\obj\BatteryPowerProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\BatteryPowerProject\\obj\\BatteryPowerProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\BatteryPowerProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.