#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\LCDProject\LCDProject.uvproj
    Project File Date:  10/18/2011

    Output:
    Build target 'Target 1'
    assembling Startup.s...
    linking...
    .\obj\LCDProject.axf: Warning: L6665W: Neither Lib$$Request$$armlib Lib$$Request$$cpplib defined, not searching ARM libraries.
    .\obj\LCDProject.axf: Error: L6411E: No compatible library exists with a definition of startup symbol __main.
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\Config.c(9): error:  #20: identifier "RST_CLK" is undefined
    src\Config.c(28): error:  #20: identifier "PORTD" is undefined
    src\Config.c(34): error:  #20: identifier "PORTC" is undefined
    src\Config.c(44): error:  #20: identifier "SysTick" is undefined
    src\LCD.c(37): error:  #20: identifier "RST_CLK" is undefined
    src\LCD.c(39): error:  #20: identifier "PORTA" is undefined
    src\LCD.c(44): error:  #20: identifier "PORTC" is undefined
    src\LCD.c(49): error:  #20: identifier "PORTE" is undefined
    src\LCD.c(57): error:  #20: identifier "RST_CLK" is undefined
    src\LCD.c(58): error:  #20: identifier "EXT_BUS_CNTRL" is undefined
    src\LCD.c(204): error:  #20: identifier "SysTick" is undefined
    src\LCD.c(208): error:  #20: identifier "SysTick" is undefined
    src\LCD.c(213): error:  #20: identifier "SysTick" is undefined
    src\LCD.c(216): warning:  #223-D: function "NVIC_EnableIRQ" declared implicitly
    src\LCD.c(216): error:  #20: identifier "SysTick_IRQn" is undefined
    src\LCDMain.c(5): warning:  #951-D: return type of function "main" must be "int"
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\LCDMain.c(6): warning:  #951-D: return type of function "main" must be "int"
    linking...
    Program Size: Code=1416 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 1 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1416 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1356 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1356 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1356 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1364 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1368 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1396 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1396 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1396 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1400 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1400 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1404 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1404 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1404 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1424 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\LCD.c(203): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=1420 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1428 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\LCD.c(204): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=1424 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\LCD.c(203): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=1420 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\LCD.c(217): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=1516 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    src\LCD.c(219): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=1536 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1536 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1536 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1532 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1532 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDProject\\obj\\LCDProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDMain.c...
    linking...
    Program Size: Code=1512 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDProject.axf" - 0 Error(s), 0 Warning(s).