#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\CAN_2\CAN2Project.uvproj
    Project File Date:  10/27/2011

    Output:
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=780 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=848 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=848 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=848 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=848 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=848 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    src\Startup.s(183): error: A1145E: Undefined exported symbol 'I2C_Handler'
    src\Startup.s:   183 00000020     EXPORT  I2C_Handler    [WEAK]
    src\Startup.s: 1 Error, 0 Warnings
    compiling CAN2Project.c...
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=856 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=864 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=864 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=864 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=852 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    src\Startup.s(137): error: A1163E: Unknown opcode External , expecting opcode or Macro
    src\Startup.s:   137 0000000e // External Interrupts
    src\Startup.s:                   ^
    src\Startup.s: 1 Error, 0 Warnings
    compiling CAN2Project.c...
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=832 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=832 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    linking...
    Program Size: Code=832 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\CAN_2\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    src\CAN2Project.c(55): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=840 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 1 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling CAN2Project.c...
    src\CAN2Project.c(55): warning:  #111-D: statement is unreachable
    linking...
    Program Size: Code=840 RO-data=224 RW-data=12 ZI-data=8292
    ".\obj\CAN2Project.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\CAN_2\\obj\\CAN2Project.AXF"