#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\MILSTD15531.uvproj
    Project File Date:  06/15/2012

    Output:
    Build target 'Target 1'
    assembling Startup.s...
    compiling MILSTD1553Main.c...
    compiling Config.c...
    linking...
    Program Size: Code=1564 RO-data=224 RW-data=20 ZI-data=8292
    ".\obj\MILSTD15531.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.306V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling MILSTD1553Main.c...
    compiling Config.c...
    src\Config.c(56): warning:  #9-D: nested comment is not allowed
    linking...
    Program Size: Code=1532 RO-data=224 RW-data=20 ZI-data=8292
    ".\obj\MILSTD15531.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.313V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling MILSTD1553Main.c...
    compiling Config.c...
    src\Config.c(56): warning:  #9-D: nested comment is not allowed
    linking...
    Program Size: Code=1532 RO-data=224 RW-data=20 ZI-data=8292
    ".\obj\MILSTD15531.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.306V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling MILSTD1553Main.c...
    compiling Config.c...
    src\Config.c(56): warning:  #9-D: nested comment is not allowed
    linking...
    Program Size: Code=1532 RO-data=224 RW-data=20 ZI-data=8292
    ".\obj\MILSTD15531.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.306V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = ?, IRPrint = 0x..000000000000000000000000
    **JLink Warning: CPU core not found.
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Load "D:\\KeilProjects\\OPORA_1986VE1\\MIL_STD_1553_1\\obj\\MILSTD15531.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\MIL_STD_1553_1\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.