Static Call Graph - [.\obj\SysTickProject2.axf]

# Static Call Graph for image .\obj\SysTickProject2.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 561]: Last Updated: Thu Jul 26 19:00:20 2012

### Maximum Stack Usage = 8 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_sh ⇒ __user_setup_stackheap

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- MIL_STD_1553B2_Handler ⇒ MIL_STD_1553B2_Handler
- MIL_STD_1553B1_Handler ⇒ MIL_STD_1553B1_Handler
- USB_Handler ⇒ USB_Handler
- CAN1_Handler ⇒ CAN1_Handler
- CAN2_Handler ⇒ CAN2_Handler
- DMA_Handler ⇒ DMA_Handler
- UART1_Handler ⇒ UART1_Handler
- UART2_Handler ⇒ UART2_Handler
- SSP1_Handler ⇒ SSP1_Handler
- BUSY_Handler ⇒ BUSY_Handler
- ARINC429R_Handler ⇒ ARINC429R_Handler
- POWER_Handler ⇒ POWER_Handler
- WWDG_Handler ⇒ WWDG_Handler
- TIMER4_Handler ⇒ TIMER4_Handler
- TIMER1_Handler ⇒ TIMER1_Handler
- TIMER2_Handler ⇒ TIMER2_Handler
- TIMER3_Handler ⇒ TIMER3_Handler
- ADC_Handler ⇒ ADC_Handler
- ETHERNET_Handler ⇒ ETHERNET_Handler
- SSP3_Handler ⇒ SSP3_Handler
- SSP2_Handler ⇒ SSP2_Handler
- ARINC429T1_Handler ⇒ ARINC429T1_Handler
- ARINC429T2_Handler ⇒ ARINC429T2_Handler
- ARINC429T3_Handler ⇒ ARINC429T3_Handler
- ARINC429T4_Handler ⇒ ARINC429T4_Handler
- BKP_Handler ⇒ BKP_Handler
- EXT_INT1_Handler ⇒ EXT_INT1_Handler
- EXT_INT2_Handler ⇒ EXT_INT2_Handler
- EXT_INT3_Handler ⇒ EXT_INT3_Handler
- EXT_INT4_Handler ⇒ EXT_INT4_Handler

  ### Function Pointers

  - ADC_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ARINC429R_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ARINC429T1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ARINC429T2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ARINC429T3_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ARINC429T4_Handler from startup.o(.text) referenced from startup.o(RESET)
  - BKP_Handler from startup.o(.text) referenced from startup.o(RESET)
  - BUSY_Handler from startup.o(.text) referenced from startup.o(RESET)
  - CAN1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - CAN2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - DMA_Handler from startup.o(.text) referenced from startup.o(RESET)
  - ETHERNET_Handler from startup.o(.text) referenced from startup.o(RESET)
  - EXT_INT1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - EXT_INT2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - EXT_INT3_Handler from startup.o(.text) referenced from startup.o(RESET)
  - EXT_INT4_Handler from startup.o(.text) referenced from startup.o(RESET)
  - HardFault_Handler from startup.o(.text) referenced from startup.o(RESET)
  - MIL_STD_1553B1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - MIL_STD_1553B2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - NMI_Handler from startup.o(.text) referenced from startup.o(RESET)
  - POWER_Handler from startup.o(.text) referenced from startup.o(RESET)
  - PendSV_Handler from startup.o(.text) referenced from startup.o(RESET)
  - Reset_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SSP1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SSP2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SSP3_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SVC_Handler from startup.o(.text) referenced from startup.o(RESET)
  - SysTick_Handler from startup.o(.text) referenced from startup.o(RESET)
  - TIMER1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - TIMER2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - TIMER3_Handler from startup.o(.text) referenced from startup.o(RESET)
  - TIMER4_Handler from startup.o(.text) referenced from startup.o(RESET)
  - UART1_Handler from startup.o(.text) referenced from startup.o(RESET)
  - UART2_Handler from startup.o(.text) referenced from startup.o(RESET)
  - USB_Handler from startup.o(.text) referenced from startup.o(RESET)
  - WWDG_Handler from startup.o(.text) referenced from startup.o(RESET)
  - __main from __main.o(!!!main) referenced from startup.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Calls]

  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup.o(.text))
  [Address Reference Count : 1]

  - startup.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  MIL_STD_1553B2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> MIL_STD_1553B2_Handler
  [Called By]
  - >> MIL_STD_1553B2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  MIL_STD_1553B1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> MIL_STD_1553B1_Handler
  [Called By]
  - >> MIL_STD_1553B1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  USB_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> USB_Handler
  [Called By]
  - >> USB_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  CAN1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> CAN1_Handler
  [Called By]
  - >> CAN1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  CAN2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> CAN2_Handler
  [Called By]
  - >> CAN2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  DMA_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> DMA_Handler
  [Called By]
  - >> DMA_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  UART1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> UART1_Handler
  [Called By]
  - >> UART1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  UART2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> UART2_Handler
  [Called By]
  - >> UART2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SSP1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SSP1_Handler
  [Called By]
  - >> SSP1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  BUSY_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> BUSY_Handler
  [Called By]
  - >> BUSY_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ARINC429R_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ARINC429R_Handler
  [Called By]
  - >> ARINC429R_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  POWER_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> POWER_Handler
  [Called By]
  - >> POWER_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  WWDG_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> WWDG_Handler
  [Called By]
  - >> WWDG_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  TIMER4_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> TIMER4_Handler
  [Called By]
  - >> TIMER4_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  TIMER1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> TIMER1_Handler
  [Called By]
  - >> TIMER1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  TIMER2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> TIMER2_Handler
  [Called By]
  - >> TIMER2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  TIMER3_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> TIMER3_Handler
  [Called By]
  - >> TIMER3_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ADC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ADC_Handler
  [Called By]
  - >> ADC_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ETHERNET_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ETHERNET_Handler
  [Called By]
  - >> ETHERNET_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SSP3_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SSP3_Handler
  [Called By]
  - >> SSP3_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  SSP2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> SSP2_Handler
  [Called By]
  - >> SSP2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ARINC429T1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ARINC429T1_Handler
  [Called By]
  - >> ARINC429T1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ARINC429T2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ARINC429T2_Handler
  [Called By]
  - >> ARINC429T2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ARINC429T3_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ARINC429T3_Handler
  [Called By]
  - >> ARINC429T3_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  ARINC429T4_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> ARINC429T4_Handler
  [Called By]
  - >> ARINC429T4_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  BKP_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> BKP_Handler
  [Called By]
  - >> BKP_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  EXT_INT1_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> EXT_INT1_Handler
  [Called By]
  - >> EXT_INT1_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  EXT_INT2_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> EXT_INT2_Handler
  [Called By]
  - >> EXT_INT2_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  EXT_INT3_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> EXT_INT3_Handler
  [Called By]
  - >> EXT_INT3_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  EXT_INT4_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup.o(.text))
  [Calls]

  - >> EXT_INT4_Handler
  [Called By]
  - >> EXT_INT4_Handler
  [Address Reference Count : 1]
  - startup.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  SysTickInit (Thumb, 12 bytes, Stack size 0 bytes, systickproject2.o(.text))
  [Called By]

  - >> main

  PortConfig (Thumb, 22 bytes, Stack size 0 bytes, systickproject2.o(.text))
  [Called By]

  - >> main

  ClkConfig (Thumb, 66 bytes, Stack size 0 bytes, systickproject2.o(.text))
  [Called By]

  - >> main

  main (Thumb, 54 bytes, Stack size 0 bytes, systickproject2.o(.text))
  [Calls]

  - >> ClkConfig
  - >> PortConfig
  - >> SysTickInit
  [Called By]
  - >> __rt_entry_main

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  - >> _call_atexit_fns (Weak Reference)
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  ### Local Symbols

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit