#

##

##

    µVision Build Log
    Project:
    D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\LCDGraphicProject.uvproj
    Project File Date:  10/21/2011

    Output:
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1356 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1384 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          0
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1384 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1384 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1384 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1384 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=1356 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(8): error:  #92: identifier-list parameters may only be used in a function definition
    src\LCDGraphic.c(9): error:  #92: identifier-list parameters may only be used in a function definition
    src\LCDGraphic.c(10): error:  #92: identifier-list parameters may only be used in a function definition
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(170): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(170): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(187): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(188): error:  #140: too many arguments in function call
    src\LCDGraphic.c(189): warning:  #223-D: function "ReadByteLCD" declared implicitly
    src\LCDGraphic.c(191): error:  #20: identifier "MyLCD" is undefined
    src\LCDGraphic.c(192): error:  #140: too many arguments in function call
    src\LCDGraphic.c(194): warning:  #223-D: function "WriteByteLCD" declared implicitly
    src\LCDGraphic.c(205): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(205): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(205): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(207): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(226): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(226): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(226): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(228): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(248): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(248): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(248): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(248): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(306): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(306): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(306): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(311): warning:  #223-D: function "GetOffset" declared implicitly
    src\LCDGraphic.c(312): warning:  #223-D: function "WriteByteLCD" declared implicitly
    src\LCDGraphic.c(312): error:  #20: identifier "Font_6x8_Data" is undefined
    src\LCDGraphic.c(326): warning:  #223-D: function "GetOffset" declared implicitly
    src\LCDGraphic.c(327): warning:  #223-D: function "WriteByteLCD" declared implicitly
    src\LCDGraphic.c(327): error:  #20: identifier "Font_6x8_Data" is undefined
    src\LCDGraphic.c(348): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(348): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(348): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(348): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(348): error:  #20: identifier "u8" is undefined
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(8): error:  #92: identifier-list parameters may only be used in a function definition
    src\LCDGraphic.c(9): error:  #92: identifier-list parameters may only be used in a function definition
    src\LCDGraphic.c(10): error:  #92: identifier-list parameters may only be used in a function definition
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(172): warning:  #550-D: variable "Crystal" was set but never used
    src\LCDGraphic.c(270): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(271): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(272): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(273): error:  #140: too many arguments in function call
    src\LCDGraphic.c(274): error:  #140: too many arguments in function call
    src\LCDGraphic.c(277): warning:  #223-D: function "WriteByteLCD" declared implicitly
    src\LCDGraphic.c(336): error:  #36: the #if for this directive is missing
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(172): warning:  #550-D: variable "Crystal" was set but never used
    src\LCDGraphic.c(270): error:  #20: identifier "u8" is undefined
    src\LCDGraphic.c(271): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(272): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(273): error:  #140: too many arguments in function call
    src\LCDGraphic.c(274): error:  #140: too many arguments in function call
    src\LCDGraphic.c(277): warning:  #223-D: function "WriteByteLCD" declared implicitly
    src\LCDGraphic.c(336): error:  #36: the #if for this directive is missing
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(172): warning:  #550-D: variable "Crystal" was set but never used
    src\LCDGraphic.c(271): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(272): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(277): warning:  #223-D: function "WriteByteLCD" declared implicitly
    src\LCDGraphic.c(336): error:  #36: the #if for this directive is missing
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(172): warning:  #550-D: variable "Crystal" was set but never used
    src\LCDGraphic.c(271): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(272): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(277): warning:  #223-D: function "WriteByteLCD" declared implicitly
    linking...
    .\obj\LCDGraphicProject.axf: Error: L6218E: Undefined symbol WriteByteLCD (referred from lcdgmain.o).
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(172): warning:  #550-D: variable "Crystal" was set but never used
    src\LCDGraphic.c(269): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(270): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(275): warning:  #223-D: function "WriteByteLCD" declared implicitly
    linking...
    .\obj\LCDGraphicProject.axf: Error: L6218E: Undefined symbol WriteByteLCD (referred from lcdgmain.o).
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(172): warning:  #550-D: variable "Crystal" was set but never used
    src\LCDGraphic.c(269): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(270): warning:  #188-D: enumerated type mixed with another type
    linking...
    Program Size: Code=1880 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 5 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGraphic.c(259): warning:  #188-D: enumerated type mixed with another type
    src\LCDGraphic.c(260): warning:  #188-D: enumerated type mixed with another type
    linking...
    Program Size: Code=1736 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 4 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1736 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1736 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1736 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1792 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1780 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1780 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    linking...
    Program Size: Code=1780 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(22): warning:  #177-D: variable "Xc" was declared but never referenced
    src\LCDGraphic.c(22): warning:  #177-D: variable "Yc" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "i" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "j" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "time" was declared but never referenced
    linking...
    Program Size: Code=1784 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 5 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(43): error:  #20: identifier "b" is undefined
    src\LCDGraphic.c(55): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(62): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(73): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(80): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(93): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(99): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(104): warning:  #223-D: function "PutPixel" declared implicitly
    src\LCDGraphic.c(23): warning:  #177-D: variable "Temp" was declared but never referenced
    src\LCDGraphic.c(230): error:  #159: declaration is incompatible with previous "PutPixel" (declared at line 55)
    src\LCDGMain.c(9): warning:  #177-D: variable "i" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "j" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "time" was declared but never referenced
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(10): error:  #141-D: unnamed prototyped parameters not allowed when body is present
    src\LCDGraphic.c(20): error:  #130: expected a "{"
    src\LCDGraphic.c(25): error:  #20: identifier "x1" is undefined
    src\LCDGraphic.c(25): error:  #20: identifier "x0" is undefined
    src\LCDGraphic.c(29): error:  #20: identifier "y1" is undefined
    src\LCDGraphic.c(29): error:  #20: identifier "y0" is undefined
    src\LCDGraphic.c(23): warning:  #177-D: variable "Temp" was declared but never referenced
    src\LCDGraphic.c(230): error:  #247: function "PutPixel" has already been defined
    src\LCDGMain.c(9): warning:  #177-D: variable "i" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "j" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "time" was declared but never referenced
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "Temp" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "i" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "j" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "time" was declared but never referenced
    linking...
    Program Size: Code=2376 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 4 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "Temp" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "i" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "j" was declared but never referenced
    src\LCDGMain.c(9): warning:  #177-D: variable "time" was declared but never referenced
    linking...
    Program Size: Code=2376 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 4 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "Temp" was declared but never referenced
    linking...
    Program Size: Code=2376 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2376 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2436 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2388 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2388 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(208): warning:  #223-D: function "DrawHorizontalLine" declared implicitly
    src\LCDGraphic.c(215): warning:  #223-D: function "DrawVerticalLine" declared implicitly
    src\LCDGraphic.c(23): warning:  #550-D: variable "flag" was set but never used
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    src\LCDGraphic.c(246): error:  #159: declaration is incompatible with previous "DrawVerticalLine" (declared at line 215)
    src\LCDGraphic.c(267): error:  #159: declaration is incompatible with previous "DrawHorizontalLine" (declared at line 208)
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #550-D: variable "flag" was set but never used
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2544 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2392 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(68): error:  #127: expected a statement
    src\LCDGraphic.c(86): warning:  #12-D: parsing restarts here after previous syntax error
    src\LCDGraphic.c(23): warning:  #550-D: variable "flag" was set but never used
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #550-D: variable "flag" was set but never used
    linking...
    Program Size: Code=2312 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2164 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(33): error:  #20: identifier "HeightHeight" is undefined
    src\LCDGraphic.c(23): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2164 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2164 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.280V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(23): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(23): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2164 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #550-D: variable "Xc" was set but never used
    src\LCDGraphic.c(24): warning:  #550-D: variable "Yc" was set but never used
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(24): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2164 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 4 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #550-D: variable "Xc" was set but never used
    src\LCDGraphic.c(24): warning:  #550-D: variable "Yc" was set but never used
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(24): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2212 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 4 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    linking...
    Program Size: Code=2308 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    linking...
    Program Size: Code=2308 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    linking...
    Program Size: Code=2308 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(24): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2604 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #177-D: variable "flag" was declared but never referenced
    src\LCDGraphic.c(24): warning:  #550-D: variable "b" was set but never used
    linking...
    Program Size: Code=2592 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 2 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGraphic.c(24): warning:  #177-D: variable "k" was declared but never referenced
    linking...
    Program Size: Code=2548 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2548 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGMain.c(7): warning:  #1295-D: Deprecated declaration DrawWindow - give arg types
    linking...
    Program Size: Code=2540 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 1 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2540 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2568 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2620 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2640 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2640 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2640 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2640 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2700 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=2768 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3040 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3040 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3048 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    ***JLink Error: Bad JTAG communication: Write to IR: Expected 0x1, got 0x0 (TAP Command : 10) @ Off 0x5.
    * JLink Info: CPU did not halt, trying to disable WDT.
    ***JLink Error: Failed to halt CPU
    ***JLink Error: Can not read register 15 (R15) while CPU is running
    Programming Failed!
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3028 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    src\LCDGMain.c(24): error:  #165: too few arguments in function call
    Target not created
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3256 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3256 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3292 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3344 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3848 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.267V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.
    Build target 'Target 1'
    assembling Startup.s...
    compiling LCDGMain.c...
    linking...
    Program Size: Code=3960 RO-data=224 RW-data=8 ZI-data=8288
    ".\obj\LCDGraphicProject.axf" - 0 Error(s), 0 Warning(s).
    Load "D:\\KeilProjects\\OPORA_1986VE1\\LCDGraphicProject\\obj\\LCDGraphicProject.AXF"
    Set JLink Project File to "D:\KeilProjects\OPORA_1986VE1\LCDGraphicProject\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.20c, compiled Sep 24 2010 19:46:42
    Firmware: J-Link ARM V7 compiled Sep  6 2010 10:43:31
    Hardware: V7.00
    S/N : 11111117
    Feature(s) : RDI, FlashBP, FlashDL, JFlash, GDBFull

    * JLink Info: TotalIRLen = 4, IRPrint = 0x01
    * JLink Info: Found Cortex-M1 r0p0, Little endian.
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF000

    Target info:
    ------------
    Device: Cortex-M1
    VTarget = 3.274V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Full Chip Erase Done.
    Programming Done.