  /**
  @addtogroup ARINC429_VE3 ARINC429 for MDR1986VE3 evaluation board
  @latexonly
  @verbatim
  ******************** (C) COPYRIGHT 2024 Milandr ******************************
  * @file    readme.txt
  * @author  Milandr Application Team
  * @version V2.0.2
  * @date    08/11/2024
  * @brief   Description of the ARINC Example.
  ******************************************************************************
  * THE PRESENT FIRMWARE IS FOR GUIDANCE ONLY. IT AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING MILANDR'S PRODUCTS IN ORDER TO FACILITATE
  * THE USE AND SAVE TIME. MILANDR SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES RESULTING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR A USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
  @endlatexonly

@par Example Description

This example provides a description of how to set a communication with the ARINC.
The ARINC transmitter send the data array and the ARINC receiver take the data
in the interrupt on presence of of data in the FIFO.
The received frame is checked and LED1 light up to indicate what the 
communication was successful, else LED2 light up.


@par Directory contains:

  - main.c               Main program


@par Hardware and Software environment:

    - This example is intended to run on MDR1986VE3 eval board with MDR1986VE3 microcontroller.
    - Pin PB0 must be connected to pin PH10.
    - Pin PB1 must be connected to pin PH11.
    - VD7 jamper must be enable.
    - VD8 jamper must be enable.
    - Depending on the configuration, HSE or LSE oscillators are used so they should be present.


@par How to use.

To launch the example, you must do the following:
    - Create a project and setup all project configurations.
    - Add main.c file.
    - Add the required files from "Libraries" folder:
        MDR32F9Qx_config.h
        MDR32F9Qx_port.c
        MDR32F9Qx_rst_clk.c
        MDR32F9Qx_eeprom.c
        MDR32F9Qx_utils.c
        MDR32F9Qx_bkp.c
        MDR32F9Qx_arinc429r.c
        MDR32F9Qx_arinc429t.c
        MDR32F9Qx_uart.c
    - Edit the MDR32F9Qx_config.h to set appropriate run-time parameter checking level.
    - Compile and link together all .c files and load your image into the target board.
    - Run the example.

 * <h3><center>&copy; COPYRIGHT 2024 Milandr</center></h3>
 */

