  /**
  @addtogroup Ethernet_X2 Ethernet_X2 for MDR1986VE3 Evaluation Board
  @latexonly
  @verbatim
  ******************** (C) COPYRIGHT 2024 Milandr ***********************************
  * @file    readme.txt
  * @author  Milandr Application Team
  * @version V2.0.2
  * @date    08/11/2024
  * @brief   Description of the Ethernet_X2 Example.
  ******************************************************************************
  * THE PRESENT FIRMWARE IS FOR GUIDANCE ONLY. IT AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING MILANDR'S PRODUCTS IN ORDER TO FACILITATE
  * THE USE AND SAVE TIME. MILANDR SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES RESULTING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR A USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
  @endlatexonly

@par Example Description

This example shows how to establish communication between two Ethernet controllers.
In case of successful packet reception ETHERNET1 lights up LED VD5 (PC0), and ETHERNET2 lights up LED VD6 (PC1).


@par Directory contains:

    - main.c               Main program


@par Hardware and Software environment:

    - This example is intended to run on MDR1986VE3 eval board with MDR1986VE3 microcontroller.
    - The example uses macros. If you want the formed packet to send Ethernet 1, then declare the "Send_ETH1" macro - similarly for the Ethernet 2.
    - Use a crossover cable to connect two Ethernet!
    - HSE and HSE2 oscillators are used so they should be present.


@par How to use.

To launch the example, you must do the following:
    - Create a project and setup all project configurations.
    - Add main.c file.
    - Add the required files from "Libraries" folder:
        MDR32F9Qx_config.h
        MDR32F9Qx_port.c
        MDR32F9Qx_rst_clk.c
        MDR32F9Qx_eth.c
        MDR32F9Qx_dma.c
        MDR32F9Qx_bkp.c
        MDR32F9Qx_eeprom.c
        MDR32F9Qx_utils.c
    - Edit the MDR32F9Qx_config.h to set appropriate run-time parameter checking level.
    - Compile and link together all .c files and load your image into the target board.
    - Run the example.

 * <h3><center>&copy; COPYRIGHT 2024 Milandr</center></h3>
 */

