  /**
  \addtogroup rtc readme
  @{
  @latexonly
  @verbatim
  ******************** (C) COPYRIGHT 2026 Milandr ******************************
  * @file    readme.txt
  * @author  Milandr Application Team
  * @version V1.0.2
  * @date    28/01/2021
  * @brief   Description of the rtc Example.
  ******************************************************************************
  * THE PRESENT FIRMWARE IS FOR GUIDANCE ONLY. IT AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING MILANDR'S PRODUCTS IN ORDER TO FACILITATE
  * THE USE AND SAVE TIME. MILANDR SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES RESULTING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR A USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
  @endlatexonly
@par Example Description

This example shows, how to use RTC.
In this demo there are RTC initialisation function, setting Date and Time functions and getting Date and Time functions. 
The results user can watch as time and date in debug mode.

@par Directory contains:

  - main.c              Main program

@par Hardware and Software environment:

  - This example is intended to run on MDR1986VK01 demo board with MDR1986VK01
  microcontroller.

@par How to use.

To launch the example, you must do the following:
  - Create a project and setup all project configurations.
  - Add main.c file.
  - Add the required files from "Libraries" folder:
        MDR1986VK01_port.h
        MDR1986VK01_clk.h
        demoboard.h
        rtc.h
        
  - Edit the MDR1986VK01_config.h to set appropriate run-time parameter checking level.
  - Compile and link together all .c files and load your image into the target board.
  - Run the example.

 * <h3><center>&copy; COPYRIGHT 2026 Milandr</center></h3>
 */

