  /**
  @addtogroup MIL_STD_1553_1T_6 MIL_STD_1553 Terminal Device for MDR1986VE1T rev. 6 Evaluation Board
  @latexonly
  @verbatim
  ******************** (C) COPYRIGHT 2026 Milandr ******************************
  * @file    readme.txt
  * @author  Milandr Application Team - Dyachkov Petr
  * @version V2.0.1
  * @date    08/11/2024
  * @brief   Description work of MIL_STD_1553 in Terminal Device mode.
  ******************************************************************************
  * THE PRESENT FIRMWARE IS FOR GUIDANCE ONLY. IT AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING MILANDR'S PRODUCTS IN ORDER TO FACILITATE
  * THE USE AND SAVE TIME. MILANDR SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES RESULTING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR A USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
  @endlatexonly

@par Example Description

This example is intended to show the functionality of microcontroller 1986VE1T
in TERMINAL mode of the standart GOST R 52070-2003.

This code write to microcontroller 1986VE1T rev. 6. In other
revision of MCU this code may performed with distinctions.


@par Directory contains:

    - main.c               Main program


@par Hardware and Software environment:

    - This example is intended to run on MDR1986VE1T eval board with MDR1986VE1T microcontroller.
    - HSE oscillator is used so it should be present.


@par How to use.

To launch the example, you must do the following:
    - Create a project and setup all project configurations.
    - Add main.c file.
    - Edit the MDR32F9Qx_config.h to set appropriate run-time parameter checking level.
    - Compile and link together all .c files and load your image into the target board.
    - Run the example.

 * <h3><center>&copy; COPYRIGHT 2026 Milandr</center></h3>
 */

