  /**
  @addtogroup Ethernet_IT Ethernet for MDR1986VE1T evaluation board
  @latexonly
  @verbatim
  ******************** (C) COPYRIGHT 2026 Milandr ******************************
  * @file    readme.txt
  * @author  Milandr Application Team
  * @version V2.1.1
  * @date    08/11/2024
  * @brief   Description of the Ethernet Example.
  ******************************************************************************
  * THE PRESENT FIRMWARE IS FOR GUIDANCE ONLY. IT AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING MILANDR'S PRODUCTS IN ORDER TO FACILITATE
  * THE USE AND SAVE TIME. MILANDR SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES RESULTING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR A USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
  @endlatexonly

@par Example Description

This example contain:
  - the example of ICMP echo server.
  - the example of TELNET echo server.


@par Directory contains:

    - src/main.c                Main program.
    - src/tcpip.c               Functions for processing ethernet frames.
    - src/hash.c                Functions for HASH calculations.
    - inc/tcpip.h               Functions prototypes for the TCPIP.
    - inc/hash.h                Functions prototypes for HASH calculations.


@par Hardware and Software environment:

    - This example is intended to run on MDR1986VE1T eval board with MDR1986VE1T microcontroller.
    - HSE and HSE2 oscillators are used so they should be present.

@par How to use.

To launch the example, you must do the following:
    - Create a project and setup all project configurations.
    - Add main.c file.
    - Add the required files from "Libraries" folder:
        MDR32F9Qx_config.h
        MDR32F9Qx_port.c
        MDR32F9Qx_rst_clk.c
        MDR32F9Qx_eth.c
        MDR32F9Qx_timer.c
        MDR32F9Qx_eeprom.c
        MDR32F9Qx_utils.c
        MDR32F9Qx_bkp.c
        MDR32F9Qx_uart.c
    - Edit the MDR32F9Qx_config.h to set appropriate run-time parameter checking level.
    - Place EEPROM functions in RAM by defining section "EXECUTABLE_MEMORY_SECTION" as RAM section.
    - Compile and link together all .c files and load your image into the target board.
    - Run the example.
If used FIFO mode, config scatter file to enable DMA.


 * <h3><center>&copy; COPYRIGHT 2026 Milandr</center></h3>
 */

