  /**
  @addtogroup ADCIU_Interrupt ADCIU_Interrupt for MDR1986BE4 evaluation board
  @latexonly
  @verbatim
  ******************** (C) COPYRIGHT 2026 Milandr ******************************
  * @file    readme.txt
  * @author  Milandr Application Team
  * @version V2.0.3
  * @date    08/11/2024
  * @brief   Description of the ADCIU_Interrupt Example.
  ******************************************************************************
  * THE PRESENT FIRMWARE IS FOR GUIDANCE ONLY. IT AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING MILANDR'S PRODUCTS IN ORDER TO FACILITATE
  * THE USE AND SAVE TIME. MILANDR SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES RESULTING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR A USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
  @endlatexonly

@par Example Description

This example describes how to use the ADCIU and interrupt to transfer
converted data from ADCIU to memory. The ADCIU is configured to converts
continuously ADC channel1. Each time an end of conversion occurs
the interrupt, the converted data from ADCIU RESULT register to the
ADCIU_data[] array of variables.


@par Directory contains:

    - main.c           Main program


@par Hardware and Software environment:

    - This example is intended to run on MDR1986BE4 eval board with MDR1986BE4 microcontroller.
    - HSE oscillator is used so it should be present.


@par How to use.

To launch the example, you must do the following:
    - Create a project and setup all project configurations.
    - Add main.c file.
    - Add the required files from "Libraries" folder:
        MDR32F9Qx_config.h
        MDR32F9Qx_port.c
        MDR32F9Qx_rst_clk.c
        MDR32F9Qx_adciu.c
        MDR32F9Qx_eeprom.c
        MDR32F9Qx_utils.c
        MDR32F9Qx_bkp.c
    - Edit the MDR32F9Qx_config.h to set appropriate run-time parameter checking level.
    - Compile and link together all .c files and load your image into the target board.
    - Run the example.


 * <h3><center>&copy; COPYRIGHT 2026 Milandr</center></h3>
 */

